/* -*- Mode: Text -*- */

autogen definitions options;

#include autogen-version.def
#include copyright.def

prog-name      = "ntpdc";
prog-title     = "vendor-specific NTPD control program";
argument       = '[ host ...]';

#include homerc.def

flag = {
    name      = ipv4;
    value     = 4;
    flags-cant = ipv6;
    descrip   = "Force IPv4 DNS name resolution";
    doc = <<-  _EndOfDoc_
	Force DNS resolution of following host names on the command line
	to the IPv4 namespace.
	_EndOfDoc_;
};

flag = {
    name      = ipv6;
    value     = 6;
    flags-cant = ipv4;
    descrip   = "Force IPv6 DNS name resolution";
    doc = <<-  _EndOfDoc_
	Force DNS resolution of following host names on the command line
	to the IPv6 namespace.
	_EndOfDoc_;
};

flag = {
    name      = command;
    value     = c;
    arg-type  = string;
    descrip   = "run a command and exit";
    max       = NOLIMIT;
    arg-name  = cmd;
    stack-arg;
    doc = <<-  _EndOfDoc_
	The following argument is interpreted as an interactive format command
	and is added to the list of commands to be executed on the specified
	host(s).
	_EndOfDoc_;
};

#include debug-opt.def

flag = {
    name      = interactive;
    value     = i;
    flags-cant = command, listpeers, peers, showpeers;
    descrip   = "Force ntpq to operate in interactive mode";
    doc = <<-  _EndOfDoc_
	Force ntpq to operate in interactive mode.  Prompts will be written
	to the standard output and commands read from the standard input.
	_EndOfDoc_;
};

flag = {
    name      = listpeers;
    value     = l;
    descrip   = "Print a list of the peers";
    flags-cant = command;
    doc = <<-  _EndOfDoc_
	Print a list of the peers known to the server as well as a summary of
	their state. This is equivalent to the 'listpeers' interactive command.
	_EndOfDoc_;
};

flag = {
    name      = numeric;
    value     = n;
    descrip   = "numeric host addresses";
    doc = <<-  _EndOfDoc_
	Output all host addresses in dotted-quad numeric format rather than
	converting to the canonical host names. 
	_EndOfDoc_;
};

flag = {
    name      = peers;
    value     = p;
    descrip   = "Print a list of the peers";
    flags-cant = command;
    doc = <<-  _EndOfDoc_
	Print a list of the peers known to the server as well as a summary
	of their state. This is equivalent to the 'peers' interactive command.
	_EndOfDoc_;
};

flag = {
    name      = showpeers;
    value     = s;
    descrip   = "Show a list of the peers";
    flags-cant = command;
    doc = <<-  _EndOfDoc_
	Print a list of the peers known to the server as well as a summary
	of their state. This is equivalent to the 'dmpeers' interactive command.
	_EndOfDoc_;
};

flag = {
    name      = unconnected;
    value     = u;
    descrip   = "Use unconnected UDP to communicate with ntpd (default on Windows)";
    doc = <<-  _EndOfDoc_
	Open an unconnected UDP association to ntpd (the default
	on Windows).
	_EndOfDoc_;
};

/* explain: Additional information whenever the usage routine is invoked */
explain = <<- _END_EXPLAIN
	_END_EXPLAIN;

doc-section	= {
  ds-type	= 'DESCRIPTION';
  ds-format	= 'mdoc';
  ds-text	= <<-  _END_PROG_MDOC_DESCRIP
.Nm
is deprecated.
Please use
.Xr ntpq 1ntpqmdoc instead - it can do everything
.Nm
used to do, and it does so using a much more sane interface.
.Pp
.Nm
is a utility program used to query
.Xr ntpd 1ntpdmdoc
about its
current state and to request changes in that state.
It uses NTP mode 7 control message formats described in the source code.
The program may
be run either in interactive mode or controlled using command line
arguments.
Extensive state and statistics information is available
through the
.Nm
interface.
In addition, nearly all the
configuration options which can be specified at startup using
ntpd's configuration file may also be specified at run time using
.Nm .
	_END_PROG_MDOC_DESCRIP;
};


doc-section	= {
  ds-type	= 'USAGE';
  ds-format     = 'mdoc';
  ds-text       = <<-  _END_MDOC_USAGE
If one or more request options are included on the command line
when
.Nm
is executed, each of the requests will be sent
to the NTP servers running on each of the hosts given as command
line arguments, or on localhost by default.
If no request options
are given,
.Nm
will attempt to read commands from the
standard input and execute these on the NTP server running on the
first host given on the command line, again defaulting to localhost
when no other host is specified.
The
.Nm
utility will prompt for
commands if the standard input is a terminal device.
.Pp
The
.Nm
utility uses NTP mode 7 packets to communicate with the
NTP server, and hence can be used to query any compatible server on
the network which permits it.
Note that since NTP is a UDP protocol
this communication will be somewhat unreliable, especially over
large distances in terms of network topology.
The
.Nm
utility makes
no attempt to retransmit requests, and will time requests out if
the remote host is not heard from within a suitable timeout
time.
.Pp
The operation of
.Nm
are specific to the particular
implementation of the
.Xr ntpd 1ntpdmdoc
daemon and can be expected to
work only with this and maybe some previous versions of the daemon.
Requests from a remote
.Nm
utility which affect the
state of the local server must be authenticated, which requires
both the remote program and local server share a common key and key
identifier.
.Pp
Note that in contexts where a host name is expected, a
.Fl 4
qualifier preceding the host name forces DNS resolution to the IPv4 namespace,
while a
.Fl 6
qualifier forces DNS resolution to the IPv6 namespace.
Specifying a command line option other than
.Fl i
or
.Fl n
will cause the specified query (queries) to be sent to
the indicated host(s) immediately.
Otherwise,
.Nm
will
attempt to read interactive format commands from the standard
input.
.Ss "Interactive Commands"
Interactive format commands consist of a keyword followed by zero
to four arguments.
Only enough characters of the full keyword to
uniquely identify the command need be typed.
The output of a
command is normally sent to the standard output, but optionally the
output of individual commands may be sent to a file by appending a
.Ql \&> ,
followed by a file name, to the command line.
.Pp
A number of interactive format commands are executed entirely
within the
.Nm
utility itself and do not result in NTP
mode 7 requests being sent to a server.
These are described
following.
.Bl -tag -width indent
.It Ic \&? Ar command_keyword
.It Ic help Ar command_keyword
A
.Sq Ic \&?
will print a list of all the command
keywords known to this incarnation of
.Nm .
A
.Sq Ic \&?
followed by a command keyword will print function and usage
information about the command.
This command is probably a better
source of information about
.Xr ntpq 1ntpqmdoc
than this manual
page.
.It Ic delay Ar milliseconds
Specify a time interval to be added to timestamps included in
requests which require authentication.
This is used to enable
(unreliable) server reconfiguration over long delay network paths
or between machines whose clocks are unsynchronized.
Actually the
server does not now require timestamps in authenticated requests,
so this command may be obsolete.
.It Ic host Ar hostname
Set the host to which future queries will be sent.
Hostname may
be either a host name or a numeric address.
.It Ic hostnames Op Cm yes | Cm no
If
.Cm yes
is specified, host names are printed in
information displays.
If
.Cm no
is specified, numeric
addresses are printed instead.
The default is
.Cm yes ,
unless
modified using the command line
.Fl n
switch.
.It Ic keyid Ar keyid
This command allows the specification of a key number to be
used to authenticate configuration requests.
This must correspond
to a key number the server has been configured to use for this
purpose.
.It Ic quit
Exit
.Nm .
.It Ic passwd
This command prompts you to type in a password (which will not
be echoed) which will be used to authenticate configuration
requests.
The password must correspond to the key configured for
use by the NTP server for this purpose if such requests are to be
successful.
.It Ic timeout Ar milliseconds
Specify a timeout period for responses to server queries.
The
default is about 8000 milliseconds.
Note that since
.Nm
retries each query once after a timeout, the total waiting time for
a timeout will be twice the timeout value set.
.El
.Ss "Control Message Commands"
Query commands result in NTP mode 7 packets containing requests for
information being sent to the server.
These are read-only commands
in that they make no modification of the server configuration
state.
.Bl -tag -width indent
.It Ic listpeers
Obtains and prints a brief list of the peers for which the
server is maintaining state.
These should include all configured
peer associations as well as those peers whose stratum is such that
they are considered by the server to be possible future
synchronization candidates.
.It Ic peers
Obtains a list of peers for which the server is maintaining
state, along with a summary of that state.
Summary information
includes the address of the remote peer, the local interface
address (0.0.0.0 if a local address has yet to be determined), the
stratum of the remote peer (a stratum of 16 indicates the remote
peer is unsynchronized), the polling interval, in seconds, the
reachability register, in octal, and the current estimated delay,
offset and dispersion of the peer, all in seconds.
.Pp
The character in the left margin indicates the mode this peer
entry is operating in.
A
.Ql \&+
denotes symmetric active, a
.Ql \&-
indicates symmetric passive, a
.Ql \&=
means the
remote server is being polled in client mode, a
.Ql \&^
indicates that the server is broadcasting to this address, a
.Ql \&~
denotes that the remote peer is sending broadcasts and a
.Ql \&~
denotes that the remote peer is sending broadcasts and a
.Ql \&*
marks the peer the server is currently synchronizing
to.
.Pp
The contents of the host field may be one of four forms.
It may
be a host name, an IP address, a reference clock implementation
name with its parameter or
.Fn REFCLK "implementation_number" "parameter" .
On
.Ic hostnames
.Cm no
only IP-addresses
will be displayed.
.It Ic dmpeers
A slightly different peer summary list.
Identical to the output
of the
.Ic peers
command, except for the character in the
leftmost column.
Characters only appear beside peers which were
included in the final stage of the clock selection algorithm.
A
.Ql \&.
indicates that this peer was cast off in the falseticker
detection, while a
.Ql \&+
indicates that the peer made it
through.
A
.Ql \&*
denotes the peer the server is currently
synchronizing with.
.It Ic showpeer Ar peer_address Oo Ar ... Oc
Shows a detailed display of the current peer variables for one
or more peers.
Most of these values are described in the NTP
Version 2 specification.
.It Ic pstats Ar peer_address Oo Ar ... Oc
Show per-peer statistic counters associated with the specified
peer(s).
.It Ic clockstat Ar clock_peer_address Oo Ar ... Oc
Obtain and print information concerning a peer clock.
The
values obtained provide information on the setting of fudge factors
and other clock performance information.
.It Ic kerninfo
Obtain and print kernel phase-lock loop operating parameters.
This information is available only if the kernel has been specially
modified for a precision timekeeping function.
.It Ic loopinfo Op Cm oneline | Cm multiline
Print the values of selected loop filter variables.
The loop
filter is the part of NTP which deals with adjusting the local
system clock.
The
.Sq offset
is the last offset given to the
loop filter by the packet processing code.
The
.Sq frequency
is the frequency error of the local clock in parts-per-million
(ppm).
The
.Sq time_const
controls the stiffness of the
phase-lock loop and thus the speed at which it can adapt to
oscillator drift.
The
.Sq watchdog timer
value is the number
of seconds which have elapsed since the last sample offset was
given to the loop filter.
The
.Cm oneline
and
.Cm multiline
options specify the format in which this
information is to be printed, with
.Cm multiline
as the
default.
.It Ic sysinfo
Print a variety of system state variables, i.e., state related
to the local server.
All except the last four lines are described
in the NTP Version 3 specification, RFC-1305.
.Pp
The
.Sq system flags
show various system flags, some of
which can be set and cleared by the
.Ic enable
and
.Ic disable
configuration commands, respectively.
These are
the
.Cm auth ,
.Cm bclient ,
.Cm monitor ,
.Cm pll ,
.Cm pps
and
.Cm stats
flags.
See the
.Xr ntpd 1ntpdmdoc
documentation for the meaning of these flags.
There
are two additional flags which are read only, the
.Cm kernel_pll
and
.Cm kernel_pps .
These flags indicate
the synchronization status when the precision time kernel
modifications are in use.
The
.Sq kernel_pll
indicates that
the local clock is being disciplined by the kernel, while the
.Sq kernel_pps
indicates the kernel discipline is provided by the PPS
signal.
.Pp
The
.Sq stability
is the residual frequency error remaining
after the system frequency correction is applied and is intended for
maintenance and debugging.
In most architectures, this value will
initially decrease from as high as 500 ppm to a nominal value in
the range .01 to 0.1 ppm.
If it remains high for some time after
starting the daemon, something may be wrong with the local clock,
or the value of the kernel variable
.Va kern.clockrate.tick
may be
incorrect.
.Pp
The
.Sq broadcastdelay
shows the default broadcast delay,
as set by the
.Ic broadcastdelay
configuration command.
.Pp
The
.Sq authdelay
shows the default authentication delay,
as set by the
.Ic authdelay
configuration command.
.It Ic sysstats
Print statistics counters maintained in the protocol
module.
.It Ic memstats
Print statistics counters related to memory allocation
code.
.It Ic iostats
Print statistics counters maintained in the input-output
module.
.It Ic timerstats
Print statistics counters maintained in the timer/event queue
support code.
.It Ic reslist
Obtain and print the server's restriction list.
This list is
(usually) printed in sorted order and may help to understand how
the restrictions are applied.
.It Ic monlist Op Ar version
Obtain and print traffic counts collected and maintained by the
monitor facility.
The version number should not normally need to be
specified.
.It Ic clkbug Ar clock_peer_address Oo Ar ... Oc
Obtain debugging information for a reference clock driver.
This
information is provided only by some clock drivers and is mostly
undecodable without a copy of the driver source in hand.
.El
.Ss "Runtime Configuration Requests"
All requests which cause state changes in the server are
authenticated by the server using a configured NTP key (the
facility can also be disabled by the server by not configuring a
key).
The key number and the corresponding key must also be made
known to
.Nm .
This can be done using the
.Ic keyid
and
.Ic passwd
commands, the latter of which will prompt at the terminal for a
password to use as the encryption key.
You will also be prompted
automatically for both the key number and password the first time a
command which would result in an authenticated request to the
server is given.
Authentication not only provides verification that
the requester has permission to make such changes, but also gives
an extra degree of protection again transmission errors.
.Pp
Authenticated requests always include a timestamp in the packet
data, which is included in the computation of the authentication
code.
This timestamp is compared by the server to its receive time
stamp.
If they differ by more than a small amount the request is
rejected.
This is done for two reasons.
First, it makes simple
replay attacks on the server, by someone who might be able to
overhear traffic on your LAN, much more difficult.
Second, it makes
it more difficult to request configuration changes to your server
from topologically remote hosts.
While the reconfiguration facility
will work well with a server on the local host, and may work
adequately between time-synchronized hosts on the same LAN, it will
work very poorly for more distant hosts.
As such, if reasonable
passwords are chosen, care is taken in the distribution and
protection of keys and appropriate source address restrictions are
applied, the run time reconfiguration facility should provide an
adequate level of security.
.Pp
The following commands all make authenticated requests.
.Bl -tag -width indent
.It Xo Ic addpeer Ar peer_address
.Op Ar keyid
.Op Ar version
.Op Cm prefer
.Xc
Add a configured peer association at the given address and
operating in symmetric active mode.
Note that an existing
association with the same peer may be deleted when this command is
executed, or may simply be converted to conform to the new
configuration, as appropriate.
If the optional
.Ar keyid
is a
nonzero integer, all outgoing packets to the remote server will
have an authentication field attached encrypted with this key.
If
the value is 0 (or not given) no authentication will be done.
The
.Ar version
can be 1, 2 or 3 and defaults to 3.
The
.Cm prefer
keyword indicates a preferred peer (and thus will
be used primarily for clock synchronisation if possible).
The
preferred peer also determines the validity of the PPS signal - if
the preferred peer is suitable for synchronisation so is the PPS
signal.
.It Xo Ic addserver Ar peer_address
.Op Ar keyid
.Op Ar version
.Op Cm prefer
.Xc
Identical to the addpeer command, except that the operating
mode is client.
.It Xo Ic broadcast Ar peer_address
.Op Ar keyid
.Op Ar version
.Op Cm prefer
.Xc
Identical to the addpeer command, except that the operating
mode is broadcast.
In this case a valid key identifier and key are
required.
The
.Ar peer_address
parameter can be the broadcast
address of the local network or a multicast group address assigned
to NTP.
If a multicast address, a multicast-capable kernel is
required.
.It Ic unconfig Ar peer_address Oo Ar ... Oc
This command causes the configured bit to be removed from the
specified peer(s).
In many cases this will cause the peer
association to be deleted.
When appropriate, however, the
association may persist in an unconfigured mode if the remote peer
is willing to continue on in this fashion.
.It Xo Ic fudge Ar peer_address
.Op Cm time1
.Op Cm time2
.Op Ar stratum
.Op Ar refid
.Xc
This command provides a way to set certain data for a reference
clock.
See the source listing for further information.
.It Xo Ic enable
.Oo
.Cm auth | Cm bclient |
.Cm calibrate | Cm kernel |
.Cm monitor | Cm ntp |
.Cm pps | Cm stats
.Oc
.Xc
.It Xo Ic disable
.Oo
.Cm auth | Cm bclient |
.Cm calibrate | Cm kernel |
.Cm monitor | Cm ntp |
.Cm pps | Cm stats
.Oc
.Xc
These commands operate in the same way as the
.Ic enable
and
.Ic disable
configuration file commands of
.Xr ntpd 1ntpdmdoc .
.Bl -tag -width indent
.It Cm auth
Enables the server to synchronize with unconfigured peers only
if the peer has been correctly authenticated using either public key
or private key cryptography.
The default for this flag is enable.
.It Cm bclient
Enables the server to listen for a message from a broadcast or
multicast server, as in the multicastclient command with
default address.
The default for this flag is disable.
.It Cm calibrate
Enables the calibrate feature for reference clocks.
The default for this flag is disable.
.It Cm kernel
Enables the kernel time discipline, if available.
The default for this flag is enable if support is available, otherwise disable.
.It Cm monitor
Enables the monitoring facility.
See the documentation here about the
.Cm monlist
command or further information.
The default for this flag is enable.
.It Cm ntp
Enables time and frequency discipline.
In effect, this switch opens and closes the feedback loop,
which is useful for testing.
The default for this flag is enable.
.It Cm pps
Enables the pulse-per-second (PPS) signal when frequency
and time is disciplined by the precision time kernel modifications.
See the
.Qq A Kernel Model for Precision Timekeeping
(available as part of the HTML documentation
provided in
.Pa /usr/share/doc/ntp )
page for further information.
The default for this flag is disable.
.It Cm stats
Enables the statistics facility.
See the
.Sx Monitoring Options
section of
.Xr ntp.conf 5
for further information.
The default for this flag is disable.
.El
.It Xo Ic restrict Ar address Ar mask
.Ar flag Oo Ar ... Oc
.Xc
This command operates in the same way as the
.Ic restrict
configuration file commands of
.Xr ntpd 1ntpdmdoc .
.It Xo Ic unrestrict Ar address Ar mask
.Ar flag Oo Ar ... Oc
.Xc
Unrestrict the matching entry from the restrict list.
.It Xo Ic delrestrict Ar address Ar mask
.Op Cm ntpport
.Xc
Delete the matching entry from the restrict list.
.It Ic readkeys
Causes the current set of authentication keys to be purged and
a new set to be obtained by rereading the keys file (which must
have been specified in the
.Xr ntpd 1ntpdmdoc
configuration file).
This
allows encryption keys to be changed without restarting the
server.
.It Ic trustedkey Ar keyid Oo Ar ... Oc
.It Ic untrustedkey Ar keyid Oo Ar ... Oc
These commands operate in the same way as the
.Ic trustedkey
and
.Ic untrustedkey
configuration file
commands of
.Xr ntpd 1ntpdmdoc .
.It Ic authinfo
Returns information concerning the authentication module,
including known keys and counts of encryptions and decryptions
which have been done.
.It Ic traps
Display the traps set in the server.
See the source listing for
further information.
.It Xo Ic addtrap Ar address
.Op Ar port
.Op Ar interface
.Xc
Set a trap for asynchronous messages.
See the source listing
for further information.
.It Xo Ic clrtrap Ar address
.Op Ar port
.Op Ar interface
.Xc
Clear a trap for asynchronous messages.
See the source listing
for further information.
.It Ic reset
Clear the statistics counters in various modules of the server.
See the source listing for further information.
.El
	_END_MDOC_USAGE;
};


doc-section	= {
  ds-type	= 'SEE ALSO';
  ds-format     = 'mdoc';
  ds-text       = <<-  _END_MDOC_SEEALSO
.Xr ntp.conf 5 ,
.Xr ntpd 1ntpdmdoc
.Rs
.%A David L. Mills
.%T Network Time Protocol (Version 3)
.%O RFC1305
.Re
	_END_MDOC_SEEALSO;
};


doc-section	= {
  ds-type	= 'AUTHORS';
  ds-format     = 'mdoc';
  ds-text       = <<-  _END_MDOC_AUTHORS
The formatting directives in this document came from FreeBSD.
	_END_MDOC_AUTHORS;
};


doc-section	= {
  ds-type	= 'BUGS';
  ds-format     = 'mdoc';
  ds-text       = <<-  _END_MDOC_BUGS
The
.Nm
utility is a crude hack.
Much of the information it shows is
deadly boring and could only be loved by its implementer.
The
program was designed so that new (and temporary) features were easy
to hack in, at great expense to the program's ease of use.
Despite
this, the program is occasionally useful.
.Pp
Please report bugs to http://bugs.ntp.org .
	_END_MDOC_BUGS;
};

.
